IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-03-11T07:20:33"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1615447232 (2021-03-11T07:20:32Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "A2WMonoblocR32_AU052FYCRA(HW)" | object type "A2WMonoblocR32_AU052FYCRA(HW)" | names: "NBS_HaierEurope_AirToWtrHeatPmps_A2WMonoblocR32:A2WMonoblocR32_AU052FYCRA(HW):306788" | material: "NBS_HaierEurope_White" | property sets: COBie

Types
  IFCUNITARYEQUIPMENTTYPE "A2WMonoblocR32_AU052FYCRA(HW)" | SPLITSYSTEM | 1 occurrence | material: "NBS_HaierEurope_White" | property sets: BOS_General, NBS_Data, Pset_UnitaryEquipmentTypeCommon, Pset_ElectricalDeviceCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_70_60_37_04:Air-to-water heat pumps" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Super aqua monobloc" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 - 20 years" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "haierhvac@haier-europe.com" (IFCTEXT)
    Material = "Steel with powder coat" (IFCTEXT)
    ModelNumber = "AU052FYCRA(HW)" (IFCTEXT)
    ModelReference = "A2W Monobloc R32_AU052FYCRA(HW)" (IFCTEXT)
    Name = "AirToWaterHeatPumps_A2WMonoblocR32_AU052FYCRA-HW_HaierEurope" (IFCTEXT)
    NominalHeight = 890.0000013528 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 370.0000005624 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1045.0000015884 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "372 x 890 x 1045 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "2 years warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HaierEurope_AirToWaterHeatPumps_A2WMonoblocR32_AU052FYCRA-HW" (IFCTEXT)
    ManufacturerName = "Haier Europe" (IFCTEXT)
    ManufacturerURL = "https://www.haierhvac.eu" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/bh0svvt2" (IFCTEXT)
    NBSDescription = "Air-to-water heat pumps" (IFCTEXT)
    NBSReference = "90-40-40/320" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_70_60_37_04" (IFCTEXT)
    Uniclass2015Title = "Air-to-water heat pumps" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Accessories = "n/a" (IFCTEXT)
    CoefficientOfPerformanceMinimum = "n/a" (IFCTEXT)
    CompressorDrive = "Inverter driven" (IFCTEXT)
    CompressorSealing = "n/a" (IFCTEXT)
    CompressorType = "DC inverter twin rotary" (IFCTEXT)
    Controls = "YR-E27A" (IFCTEXT)
    CoolingCapacityAt18Degrees = "5 kW (LWT 18°C / OAT 35°C)" (IFCTEXT)
    CoolingCapacityAt7Degrees = "5 kW (LWT 7°C / OAT 35°C)" (IFCTEXT)
    CoolingPowerOutputAt18Degrees = "1 kW (LWT 18°C / OAT 35°C)" (IFCTEXT)
    CoolingPowerOutputAt7Degrees = "1.56 kW (LWT 7°C / OAT 35°C)" (IFCTEXT)
    ElectricalSupplyType = "1/220-240, 50/60" (IFCTEXT)
    FanConfiguration = "n/a" (IFCTEXT)
    FanFanDrive = "n/a" (IFCTEXT)
    FanType = "n/a" (IFCTEXT)
    HeatPumpType = "Air to water" (IFCTEXT)
    HeatingCapacityAt35Degrees = "5 kW (LWT 35°C / OAT 7°C)" (IFCTEXT)
    HeatingCapacityAt55Degrees = "5 kW (LWT 55°C / OAT 7°C)" (IFCTEXT)
    HeatingPowerOutputAt35Degrees = "0.99 kW (LWT 35°C / OAT 7°C)" (IFCTEXT)
    HeatingPowerOutputAt55Degrees = "1.64 kW (LWT 55°C / OAT 7°C)" (IFCTEXT)
    LeavingWaterTemperatureRangeCooling = "5 - 20°C" (IFCTEXT)
    LeavingWaterTemperatureRangeHeating = "25 - 60°C" (IFCTEXT)
    MaxRunningCurrent = "13.5 A" (IFCTEXT)
    Mode = "n/a" (IFCTEXT)
    OutdoorOperatingTemperatureRangeCooling = "10 - 46°C" (IFCTEXT)
    OutdoorOperatingTemperatureRangeHeating = "-25 - 35°C" (IFCTEXT)
    RecommendedCircuitBreaker = "30 A" (IFCTEXT)
    Refrigerant = "R32" (IFCTEXT)
    SoundPowerLevel = "59 dB" (IFCTEXT)
    StandardsElectricalSafety = "n/a" (IFCTEXT)
    StandardsSafetyAndEnvironmental = "Eurovent certified" (IFCTEXT)
    StandardsTestRequirements = "n/a" (IFCTEXT)
    WaterFlowRate = "14.3 L/min" (IFCTEXT)
    WaterPipingConnection = "RC 3/4 inch" (IFCTEXT)
    Weight = "80 kg" (IFCTEXT)
  Pset_UnitaryEquipmentTypeCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    ConductorFunction = "n/a" (IFCTEXT)
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    IK_Code = "n/a" (IFCTEXT)
    IP_Code = "n/a" (IFCTEXT)
    InsulationStandardClass = "n/a" (IFCTEXT)
    NominalFrequencyRange = "50/60 Hz" (IFCTEXT)
    NumberOfPoles = 1 (IFCINTEGER)
    PowerFactor = 0. (IFCREAL)
    RatedCurrent = "n/a" (IFCTEXT)
    RatedVoltage = "220 - 240 V" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcUnitaryEquipmentType" (IFCTEXT)
    IfcExportType = "SPLITSYSTEM" (IFCTEXT)