IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-03-11T08:28:55"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1615451335 (2021-03-11T08:28:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCDISTRIBUTIONCONTROLELEMENT | type IFCCONTROLLERTYPE "CentralisedControllerMax256ID_YCZ-A004" | object type "CentralisedControllerMax256ID_YCZ-A004" | names: "NBS_HaierEurope_CtrlPnls_CentralisedControllerMax256ID:CentralisedControllerMax256ID_YCZ-A004:341027" | material: "NBS_HaierEurope_White" | property sets: COBie

Types
  IFCCONTROLLERTYPE "CentralisedControllerMax256ID_YCZ-A004" | 1 occurrence | material: "NBS_HaierEurope_White" | property sets: BOS_General, NBS_Data, Pset_ControllerTypeCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCDISTRIBUTIONCONTROLELEMENT)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_75_50_18_51:Mechanical services control panels" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Smart controller system for medium size plants up to 256 indoor units" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 - 20 years" (IFCTEXT)
    Features = "Large 7" LCD TFT full touchscreen display, possibility of naming units and groups, built in weekly timer, displaying alarms, 32 independent cooling circuits, each with their own HA-MA164AD converter, MOD-BUS output as standard" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "haierhvac@haier-europe.com" (IFCTEXT)
    Material = "Plastic" (IFCTEXT)
    ModelNumber = "YCZ-A004" (IFCTEXT)
    ModelReference = "Centralised controller Max 256 ID_YCZ-A004" (IFCTEXT)
    Name = "ControlPanels_CentralisedControllerMax256ID_YCZ-A004_HaierEurope" (IFCTEXT)
    NominalHeight = 20.0000000304 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 125.00000019 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 190.0000002888 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangular" (IFCTEXT)
    Size = "20 x 125 x 190 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "2 years warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HaierEurope_ControlPanels_CentralisedControllerMax256ID_YCZ-A004" (IFCTEXT)
    ManufacturerName = "Haier Europe" (IFCTEXT)
    ManufacturerURL = "https://www.haierhvac.eu" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/133crntd" (IFCTEXT)
    NBSDescription = "Control panels" (IFCTEXT)
    NBSReference = "90-65-50/340" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_75_50_18_51" (IFCTEXT)
    Uniclass2015Title = "Mechanical services control panels" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    CableEntry = "Wired or wireless" (IFCTEXT)
    EnclosureColour = "White" (IFCTEXT)
    EnclosureDoorsAndPanelsForm = "n/a" (IFCTEXT)
    EnclosureDoorsAndPanelsHardware = "n/a" (IFCTEXT)
    EnclosureDoorsAndPanelsLocks = "n/a" (IFCTEXT)
    EnclosureDoorsAndPanelsSwing = "n/a" (IFCTEXT)
    EnclosureFinish = "n/a" (IFCTEXT)
    EnclosureIngressProtectionMinimum = "n/a" (IFCTEXT)
    EnclosureMaterial = "Plastic" (IFCTEXT)
    EnclosureMechanicalProtectionMinimum = "n/a" (IFCTEXT)
    GlandPlateGaskets = "n/a" (IFCTEXT)
    InterconnectingCable = "n/a" (IFCTEXT)
    InternalCableZones = "n/a" (IFCTEXT)
    InternalSeparation = "n/a" (IFCTEXT)
    IsolatorMechanicalInterlocking = "n/a" (IFCTEXT)
    IsolatorNumberOfPoles = 0 (IFCINTEGER)
    IsolatorRatedOperationalCurrentIn = "n/a" (IFCTEXT)
    IsolatorRatedOperationalFrequency = "n/a" (IFCTEXT)
    IsolatorRatedOperationalVoltageUe = "n/a" (IFCTEXT)
    IsolatorRatedShortTimeWithstandCurrentIcwFor1S = "n/a" (IFCTEXT)
    IsolatorTerminals = "n/a" (IFCTEXT)
    IsolatorType = "Controller" (IFCTEXT)
    IsolatorUtilizationCategory = "n/a" (IFCTEXT)
    TerminalsIdentificationCableTerminations = "n/a" (IFCTEXT)
    TerminalsIdentificationNeutralAndEarthBarTerminals = "n/a" (IFCTEXT)
    TerminalsMounting = "Wall mounted" (IFCTEXT)
    TrunkingMaterial = "n/a" (IFCTEXT)
    TrunkingStandard = "n/a" (IFCTEXT)
  Pset_ControllerTypeCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcControllerType" (IFCTEXT)
    IfcExportType = "NOTDEFINED" (IFCTEXT)