IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-03-11T07:21:55"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1615447315 (2021-03-11T07:21:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "MRVSDCInverterUnitWithFrontDischarge_AU60NFIERA(H)" | object type "MRVSDCInverterUnitWithFrontDischarge_AU60NFIERA(H)" | names: "NBS_HaierEurope_SpltCoilRmtAirCooldCndnsngUnits_MRVSDCInverterUnitWithFrontDischarge:MRVSDCInverterUnitWithFrontDischarge_AU60NFIERA(H):306788" | material: "NBS_HaierEurope_White" | property sets: COBie

Types
  IFCUNITARYEQUIPMENTTYPE "MRVSDCInverterUnitWithFrontDischarge_AU60NFIERA(H)" | SPLITSYSTEM | 1 occurrence | material: "NBS_HaierEurope_White" | property sets: BOS_General, NBS_Data, Pset_UnitaryEquipmentTypeCommon, Pset_UnitaryEquipmentTypeAirConditioningUnit, Pset_ElectricalDeviceCommon, IFC

Property sets
  COBie | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_70_65_03_84:Split coil remote air-cooled condensing units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "DC inverter unit with front discharge" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 - 20 years" (IFCTEXT)
    Features = "Energy efficient, side discharge and compact design, high efficiency DC fan motor, large diameter fan, high efficiency condenser, twin rotary DC inverter compressor, double pressure sensor, automatic refrigerant reclaim technology, can power up to 9 indoor units from one outdoor unit" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "haierhvac@haier-europe.com" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "AU60NFIERA(H)" (IFCTEXT)
    ModelReference = "MRV S DC Inverter Unit with Front Discharge_AU60NFIERA(H)" (IFCTEXT)
    Name = "SplitCoilRemoteAirCooledCondensingUnits_MRVSDCInverterUnitwithFrontDischarge_AU60NFIERA-H_HaierEurope" (IFCTEXT)
    NominalHeight = 1250.0000019 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 340.0000005168 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 960.0000014592 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "1250 x 960 x 340 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "2 years warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HaierEurope_SplitCoilRemoteAirCooledCondensingUnits_MRVSDCInverterUnitwithFrontDischarge_AU60NFIERA-H" (IFCTEXT)
    ManufacturerName = "Haier Europe" (IFCTEXT)
    ManufacturerURL = "https://www.haierhvac.eu" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/ijx02ya4" (IFCTEXT)
    NBSDescription = "Split coil remote air cooled condensing units" (IFCTEXT)
    NBSReference = "90-45-05/370" (IFCTEXT)
    ProductInformation = "https://www.haierhvac.eu/en/product/vrf-systems/mrv-s" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_70_65_03_84" (IFCTEXT)
    Uniclass2015Title = "Split coil remote air-cooled condensing units" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    AirFlow = "6500 m³/h" (IFCTEXT)
    Applications = "Large commercial buildings, multi-story office spaces and large homes where standard central HVAC can be inefficient all benefit from our efficient mini-split heating and cooling systems" (IFCTEXT)
    Arrangement = "n/a" (IFCTEXT)
    CasingFinish = "n/a" (IFCTEXT)
    CasingMaterial = "n/a" (IFCTEXT)
    CompressorType = "Rotary" (IFCTEXT)
    CoolingCapacity = "18 kW" (IFCTEXT)
    Duty = "n/a" (IFCTEXT)
    ElectricalSupply = "3/380-400/50/60" (IFCTEXT)
    ExternalNoiseLevel = "n/a" (IFCTEXT)
    ExternalTemperatureOperatingLimitsCooling = "-5°C - 48°C" (IFCTEXT)
    ExternalTemperatureOperatingLimitsHeating = "-15°C - 21°C" (IFCTEXT)
    IndoorOutdoorCapacityRatio = "50-130%" (IFCTEXT)
    MaximumNumberOfConnectableIUs = "9" (IFCTEXT)
    MaximumPipingLength = "150000 mm" (IFCTEXT)
    Mounting = "Wall mounted" (IFCTEXT)
    RatedPowerInputCooling = "5.19 kW" (IFCTEXT)
    RatedPowerInputHeating = "5.13 kW" (IFCTEXT)
    SoundPowerLevel = "70dB" (IFCTEXT)
    SoundPressureLevel = "59dB" (IFCTEXT)
    Standards = "Eurovent certified" (IFCTEXT)
    Weight = "99 kg" (IFCTEXT)
  Pset_UnitaryEquipmentTypeCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
  Pset_UnitaryEquipmentTypeAirConditioningUnit | properties | on 1 type object
    CondenserEnteringTemperature = 0. (IFCREAL)
    CondenserFlowrate = 0. (IFCREAL)
    CondenserLeavingTemperature = 0. (IFCREAL)
    CoolingEfficiency = 0. (IFCREAL)
    HeatingCapacity = 20. (IFCREAL)
    HeatingEfficiency = 0. (IFCREAL)
    LatentCoolingCapacity = 0. (IFCREAL)
    OutsideAirFlowrate = 0. (IFCREAL)
    SensibleCoolingCapacity = 0. (IFCREAL)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    ConductorFunction = "n/a" (IFCTEXT)
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    IK_Code = "n/a" (IFCTEXT)
    IP_Code = "n/a" (IFCTEXT)
    InsulationStandardClass = "n/a" (IFCTEXT)
    NominalFrequencyRange = "50/60 Hz" (IFCTEXT)
    NumberOfPoles = 3 (IFCINTEGER)
    PowerFactor = 0. (IFCREAL)
    RatedCurrent = "n/a" (IFCTEXT)
    RatedVoltage = "380 - 400 V" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcUnitaryEquipmentType" (IFCTEXT)
    IfcExportType = "SPLITSYSTEM" (IFCTEXT)