IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-03-11T07:24:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1615447448 (2021-03-11T07:24:08Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "2WayCassette_AB072MBERA" | object type "2WayCassette_AB072MBERA" | names: "NBS_HaierEurope_SpltCoilRoomAirCndtnngUnits_MRVIndoorUnit_2WayCassette:2WayCassette_AB072MBERA:317985" | material: "NBS_HaierEurope_White" | property sets: COBie

Types
  IFCUNITARYEQUIPMENTTYPE "2WayCassette_AB072MBERA" | SPLITSYSTEM | 1 occurrence | material: "NBS_HaierEurope_White" | property sets: BOS_General, NBS_Data, Pset_UnitaryEquipmentTypeCommon, Pset_UnitaryEquipmentTypeAirConditioningUnit, Pset_ElectricalDeviceCommon, IFC

Property sets
  COBie | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_70_65_03_86:Split coil room air conditioning units" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "2 way cassette compact unit" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 - 20 years" (IFCTEXT)
    Features = "Slim design, standard condensate drain pump, silent operation" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "haierhvac@haier-europe.com" (IFCTEXT)
    Material = "n/a" (IFCTEXT)
    ModelNumber = "AB072MBERA" (IFCTEXT)
    ModelReference = "MRV Cassette 2 Way_AB072MBERA" (IFCTEXT)
    Name = "SplitCoilRoomAirConditioningUnits_MRVCassette2Way_AB072MBERA_HaierEurope" (IFCTEXT)
    NominalHeight = 220.0000003344 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 620.0000009424 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 817.00000124184 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "870 x 620 x 220 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "2 years warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HaierEurope_SplitCoilRoomAirConditioningUnits_MRVCassette2Way_AB072MBERA" (IFCTEXT)
    ManufacturerName = "Haier Europe" (IFCTEXT)
    ManufacturerURL = "https://www.haierhvac.eu" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/wprpl1pj" (IFCTEXT)
    NBSDescription = "Split coil room air conditioning units" (IFCTEXT)
    NBSReference = "90-45-05/360" (IFCTEXT)
    ProductInformation = "https://www.haierhvac.eu/en/product/mrv/2-way-cassette" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_70_65_03_86" (IFCTEXT)
    Uniclass2015Title = "Split coil room air conditioning units" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Access = "n/a" (IFCTEXT)
    AirFlow = "840 m³/h" (IFCTEXT)
    AirVolume = "n/a" (IFCTEXT)
    CasingFinish = "n/a" (IFCTEXT)
    CondensateDrainage = "n/a" (IFCTEXT)
    Controls = "HW-BA116ABK, HW-BA101ABT, YR-E17, YR-HD01, YR-E16B" (IFCTEXT)
    CoolingCapacity = "2.2 kW" (IFCTEXT)
    CoolingLoadLatent = "n/a" (IFCTEXT)
    CoolingLoadSensible = "n/a" (IFCTEXT)
    CoolingLoadTotal = "n/a" (IFCTEXT)
    ElectricalSupply = "1/220-230/50/60" (IFCTEXT)
    Filters = "n/a" (IFCTEXT)
    Grille = "n/a" (IFCTEXT)
    HeaterBattery = "n/a" (IFCTEXT)
    HeatingLoad = "n/a" (IFCTEXT)
    Humidification = "n/a" (IFCTEXT)
    Insulation = "n/a" (IFCTEXT)
    Mounting = "Ceiling mounted" (IFCTEXT)
    NumberOfCircuits = 0 (IFCINTEGER)
    PanelDimensions = "1055 x 680 x 68 mm" (IFCTEXT)
    PanelType = "P2B-1055IB" (IFCTEXT)
    PanelWeight = "8 kg" (IFCTEXT)
    Refrigerant = "n/a" (IFCTEXT)
    Resistance = "n/a" (IFCTEXT)
    SoundPowerLevel = "55/50/46 dB (A/M/B)" (IFCTEXT)
    SoundPressureLevel = "42/37/33 dB (A/M/B)" (IFCTEXT)
    Standards = "Eurovent certified" (IFCTEXT)
    Weight = "23 kg" (IFCTEXT)
  Pset_UnitaryEquipmentTypeCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
  Pset_UnitaryEquipmentTypeAirConditioningUnit | properties | on 1 type object
    CondenserEnteringTemperature = 0. (IFCREAL)
    CondenserFlowrate = 0. (IFCREAL)
    CondenserLeavingTemperature = 0. (IFCREAL)
    CoolingEfficiency = 0. (IFCREAL)
    HeatingCapacity = 2.5 (IFCREAL)
    HeatingEfficiency = 0. (IFCREAL)
    LatentCoolingCapacity = 0. (IFCREAL)
    OutsideAirFlowrate = 0. (IFCREAL)
    SensibleCoolingCapacity = 0. (IFCREAL)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    ConductorFunction = "n/a" (IFCTEXT)
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    IK_Code = "n/a" (IFCTEXT)
    IP_Code = "n/a" (IFCTEXT)
    InsulationStandardClass = "n/a" (IFCTEXT)
    NominalFrequencyRange = "50/60 Hz" (IFCTEXT)
    NumberOfPoles = 1 (IFCINTEGER)
    PowerFactor = 0. (IFCREAL)
    RatedCurrent = "n/a" (IFCTEXT)
    RatedVoltage = "220 - 230 V" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcUnitaryEquipmentType" (IFCTEXT)
    IfcExportType = "SPLITSYSTEM" (IFCTEXT)