IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-03-11T07:43:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Alternate UI 19.2.20.24"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1615448623 (2021-03-11T07:43:43Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCENERGYCONVERSIONDEVICE | type IFCUNITARYEQUIPMENTTYPE "MRVWDCInverterWaterCooled_AV08IMWEWA" | object type "MRVWDCInverterWaterCooled_AV08IMWEWA" | names: "NBS_HaierEurope_WtrToAirHeatPmps_MRVWDCInverterWaterCooled:MRVWDCInverterWaterCooled_AV08IMWEWA:335313" | material: "NBS_HaierEurope_White" | property sets: COBie

Types
  IFCUNITARYEQUIPMENTTYPE "MRVWDCInverterWaterCooled_AV08IMWEWA" | SPLITSYSTEM | 1 occurrence | material: "NBS_HaierEurope_White" | property sets: BOS_General, NBS_Data, Pset_UnitaryEquipmentTypeCommon, Pset_UnitaryEquipmentTypeAirConditioningUnit, Pset_ElectricalDeviceCommon, IFC

Property sets
  COBie | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_70_60_37_96:Water-to-air heat pumps" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "White" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Water-cooled Full DC inverter heat pump system" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 - 20 years" (IFCTEXT)
    Features = "Double coil outdoor heat exchanger, compatible with all the MRV indoor units, compact size" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "haierhvac@haier-europe.com" (IFCTEXT)
    Material = "Steel powder coated" (IFCTEXT)
    ModelNumber = "AV08IMWEWA" (IFCTEXT)
    ModelReference = "MRV W DC Inverter Water Cooled_AV08IMWEWA" (IFCTEXT)
    Name = "WaterToAirHeatPumps_MRVWDCInverterWaterCooled_AV08IMWEWA_HaierEurope" (IFCTEXT)
    NominalHeight = 995.0000015124 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 545.0000008284 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 775.000001178 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "545 x 995 x 775 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "2 years warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HaierEurope_WaterToAirHeatPumps_MRVWDCInverterWaterCooled_AV08IMWEWA" (IFCTEXT)
    ManufacturerName = "Haier Europe" (IFCTEXT)
    ManufacturerURL = "https://www.haierhvac.eu" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/ozrjbjrk" (IFCTEXT)
    NBSDescription = "Water-to-air heat pumps" (IFCTEXT)
    NBSReference = "90-40-40/350" (IFCTEXT)
    ProductInformation = "https://www.haierhvac.eu/en/product/vrf-systems/mrv-w" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_70_60_37_96" (IFCTEXT)
    Uniclass2015Title = "Water-to-air heat pumps" (IFCTEXT)
    Uniclass2015Version = "Products v1.20" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Accessories = "n/a" (IFCTEXT)
    CoefficientOfPerformanceMinimum = "n/a" (IFCTEXT)
    CompressorDrive = "Inverter driven" (IFCTEXT)
    CompressorSealing = "n/a" (IFCTEXT)
    CompressorType = "DC Inverter Scroll" (IFCTEXT)
    ConnectionType = "Internal thread" (IFCTEXT)
    ElectricalSupplyType = "3/380-400/50/60 (5 wires L1+L2+L3+N+T)" (IFCTEXT)
    ExchangerPressureDrop = "35 Kpa" (IFCTEXT)
    HeatPumpType = "Multi-split" (IFCTEXT)
    IndoorOutdoorCapacityRatio = "50 - 130%" (IFCTEXT)
    MaxAbsorbedCurrentCooling = "20.79 A" (IFCTEXT)
    MaxAbsorbedCurrentHeating = "20.79 A" (IFCTEXT)
    MaxAbsorbedPowerCooling = "13 kW" (IFCTEXT)
    MaxAbsorbedPowerHeating = "13 kW" (IFCTEXT)
    MaxWaterInputPressure = "1.6 Mpa" (IFCTEXT)
    MaximumNumberOfConnectableIUs = "13" (IFCTEXT)
    MaximumPipingLength = "300000 mm" (IFCTEXT)
    Mode = "n/a" (IFCTEXT)
    OutputCooling = "22.4 kW" (IFCTEXT)
    OutputHeating = "25 kW" (IFCTEXT)
    SoundPowerLevel = "61 dB" (IFCTEXT)
    SoundPressureLevel = "50 dB" (IFCTEXT)
    StandardsElectricalSafety = "n/a" (IFCTEXT)
    StandardsPerformance = "n/a" (IFCTEXT)
    StandardsSafetyAndEnvironmentalRequirements = "Eurovent certified" (IFCTEXT)
    StandardsTestRequirements = "n/a" (IFCTEXT)
    TransferMedium = "R410A" (IFCTEXT)
    WaterInputTemperatureRange = "7 to 45°C" (IFCTEXT)
    Weight = "183 kg" (IFCTEXT)
  Pset_UnitaryEquipmentTypeCommon | properties | on 1 type object
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
  Pset_UnitaryEquipmentTypeAirConditioningUnit | properties | on 1 type object
    CondenserEnteringTemperature = 0. (IFCREAL)
    CondenserFlowrate = 0. (IFCREAL)
    CondenserLeavingTemperature = 0. (IFCREAL)
    CoolingEfficiency = 0. (IFCREAL)
    HeatingCapacity = 25. (IFCREAL)
    HeatingEfficiency = 0. (IFCREAL)
    LatentCoolingCapacity = 0. (IFCREAL)
    OutsideAirFlowrate = 0. (IFCREAL)
    SensibleCoolingCapacity = 0. (IFCREAL)
  Pset_ElectricalDeviceCommon | properties | on 1 type object
    ConductorFunction = "n/a" (IFCTEXT)
    HasProtectiveEarth = FALSE (IFCBOOLEAN)
    IK_Code = "n/a" (IFCTEXT)
    IP_Code = "n/a" (IFCTEXT)
    InsulationStandardClass = "n/a" (IFCTEXT)
    NominalFrequencyRange = "50/60 Hz" (IFCTEXT)
    NumberOfPoles = 3 (IFCINTEGER)
    PowerFactor = 0. (IFCREAL)
    RatedCurrent = "n/a" (IFCTEXT)
    RatedVoltage = "380 - 400 V" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcUnitaryEquipmentType" (IFCTEXT)
    IfcExportType = "SPLITSYSTEM" (IFCTEXT)